# Collapsible hand post EH VS

**Single-beam entrance aid,** with design certification in accordance with DIN 19572,   
made of 1.4404 (AISI 316 L) stainless steel. Available as either a removable and portable   
or as stationary collapsible unit. Consisting of a handle and guide.

**Guide** with two holes, diameter: 12 mm, for bolted fixing to the wall of the manhole. With a   
possibility of adjustment for the handle.

**Handle** of distortion-free pipe, 33.7 x 3.6 mm, total length: 1500 mm.

Completely shielded arc welded, acid-treated in a pickling bath and passivated.

## Options:

➤ Stainless steel fixing material: stud anchors

## Special design:

➤ Suitable for ‘econorm’ manholes, wall distance to beginning of insertion opening: 158 mm