# Collapsible hand post with double handle EH VSD

# **Collapsible hand pos**t with double handle, with design certification in accordance with DIN 19572, made of 1.4307 (AISI 304 L) stainless steel, for safety access ladders with 300 mm, 400 mm, 500 mm width, for ladder lengths from 2010 mm. Overall length: 1800 mm.

Entrance aid in accordance with DIN 19572.

Access ladders must have a handhold at their exit. This requirement is deemed to be fulfilled if one or both handles of a ladder project at least 1.1 m beyond the exit height.

Ladder width = mm,

Ladder length = m

Completely shielded arc welded, acid-treated in a pickling bath and passivated.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel